**Parts List for the 450 Ω Ladder Line J-Pole for 144 and 440 MHz**

(This was posted in the October 2022 issue of QST. Pg. 38)

(5’) 450 Ω Ladder Line

(10’) RG -58 Coax

(1) PL-259 with Adapter for RG-58 or BNC Connector

Tools needed:

Tape Measure

Sharp Pocket Knife or Razor Knife

Electrical Tape

Soldering Iron

Wire Cutter (This is copper plated steel) (I will have one if you need)